|  |  |  |
| --- | --- | --- |
|  | Average Current | Peak Current |
| System | 13 Ma | 45 mA |
| MSP | 10 mA | ~ |
| Peripheral (RF) | 3.8 mA | 39 mA |
| PPG | 0.28 mA | ~ |
| Electrodes | 20 uA | ~ |